# SPI Protocol

Q. What is open-drain output signal?

It is an open-drain output signal so that <FSTAT> pins of several devices can be connected to a common pull-up resistor and one microcontroller I/O port.